CV Landsat WRS-2 PATH ROW.gpkg
Layer WRS-1

Data acquired from Landsat 1 to 3 follow the Worldwide Reference System-1 (WRS-1). Two geometric processing levels are available: L1TP (Terrain Precision Correction) and L1GS (Systematic Correction). The former provides high positional accuracy and consistent alignment between scenes, whereas the latter may exhibit positional errors on the order of tens to hundreds of meters and significant misalignments (up to tens or even hundreds of pixels) between scenes.

Cabo Verde is covered by three paths (225, 226, and 227) and three rows (048, 049, and 050). The combination of these paths and rows results in a total of seven distinct granules containing data.


Read more: 
https://www.usgs.gov/landsat-missions/landsat-shapefiles-and-kml-files


More GIS data for Cabo Verde:
https://www.nsloureiro.pt/gis-cv