CV Landsat WRS-2 PATH ROW.gpkg


Data acquired from Landsat 4 onward follow the Worldwide Reference System-2 (WRS-2). This updated system provides improved orbital geometry, enhances the positional accuracy of scenes relative to the Earth's surface, and reduces geometric distortions. The spatial dimensions of each scene are approximately 170 × 185 km.

Cabo Verde is covered by three paths (209, 210, and 211) and three rows (048, 049, and 050). The combination of these paths and rows results in a total of seven distinct granules containing data.


Read more: 
https://www.usgs.gov/landsat-missions/landsat-shapefiles-and-kml-files


More GIS data for Cabo Verde:
https://www.nsloureiro.pt/gis-cv